**Project : Modifying 1 pre-made indicator as I described**

I have a request of modifying functions in a pre-made indicator.



Image of OIH\_PA\_Lines\_v1.0\_RAW\_2303021722

**1. Update old code, please.**

**2. Fill out the blank with “0.00000”, please.**

OIH\_OA\_Lines\_v1.0\_RAW 0.00016

v2 0.00145

v3 -0.00129

v4

v5

v6

v7

v8

As you can see, there are empty values in data window, so I hope you to fill out the blank with “0.00000”.

**3. Please remove v4 and v5 if they are not necessary.**

And I don’t know exactly if v4 and v5 are necessary or not.

v4 and v5 don’t show any numerical values as always.

If 2 buffers are not necessary, then remove them, please.

**4. ISM (Inherit State Mode) of v6, v7 and v8**

v6 is for yellow bar in current indicator

v7 is for blue bar in current indicator

v8 is for white bar in current indicator

Finally new indicator will have buffers as followings below.

v1 Fast Line 0.00016 \*\* same as before

v2 Slow line 0.00145 \*\* same as before

v3 All Histogram Bars -0.00129 \*\* same as before

v4 Yellow Bar \*\* previous v6, yellow bar

v5 Blue Bar \*\* previous v7, blue bar

v6 White Bar \*\* previous v8, white bar

v7 v4 ISM \*\* ISM of v4

v8 v5 ISM \*\* ISM of v5

v9 v6 ISM \*\* ISM of v6

**5. Fix “TimeFrame” function, please.**

If I put “30” or “60”, then it does not work.

So, I hope you to check and fix the function.

**6. Remove the alert function in parameter option and the code, please.**

**7. I need “Max Bars” function**

Max Bars 500

File name of a new indicator will be **“OIH\_PA\_Lines\_v1.0”.**

**Requirement(s)**

∙ It should work properly as I described.